Known issues
	- rim:  Warning: i3d contains non-binary indexed triangle sets

Crane info to know:
	-to turn the turn table when anything is attached, you need to select control group 1

Boom info to know:
	-If just using the telescoping sections, the Hydraulic Jib or Luffing Jib reach must be set to 0m to get the correct placement of the hook cables
	-The hook must be attached with the boom as close to the hook as possible (similar to how a true hook is reaved up)
	-When the boom is folded the hook attacher joint will return to the boom.  So if you are trying to attach the hook with the boom raised and the attacher lowered and it goes too far, you can hit fold and it will return to the top.
	

Controlling the Crane:

Carrier
Control group 1 Crane
	-slew (turn) crane - AXIS_CRANE_ARM keyboard key k/m
	-raise/lower lift cylinders - AXIS_CRANE_ARM2 keyboard j/n
	-ballast plate raise/lower - AXIS_CRANE_SUPPORT keyboard lctrl + a/d
	-fold - keyboard x
	(this will bring the crane cab into operating position from the transport position if you do not want to use simple ic) 
	-steering modes 

Control group 2 front outriggers
	-rotate left front outrigger - AXIS_CRANE_ARM2 keyboard j/n
	-rotate right front outrigger - AXIS_CRANE_ARM keyboard k/m
	-extend left front outrigger - AXIS_CRANE_ARM3 keyboard lshift + j/n
	-extend right front outrigger - AXIS_CRANE_ARM4 keyboard lshift + k/m
	-lower left front outrigger - AXIS_CRANE_TOOL2 keyboard lshift + lctrl + j/n
	-lower right front outrigger - AXIS_CRANE_TOOL3 keyboard lshift + lctrl + k/m

Control group 3 rear outriggers
	-rotate left rear outrigger - AXIS_CRANE_ARM2 keyboard j/n
	-rotate right rear outrigger - AXIS_CRANE_ARM keyboard k/m
	-extend left rear outrigger - AXIS_CRANE_ARM3 keyboard lshift + j/n
	-extend right rear outrigger - AXIS_CRANE_ARM4 keyboard lshift + k/m
	-lower left rear outrigger - AXIS_CRANE_TOOL2 keyboard lshift + lctrl + j/n
	-lower right rear outrigger - AXIS_CRANE_TOOL3 keyboard lshift + lctrl + k/m

T3/T7 Boom controls
	-raise boom - AXIS_CRANE_ARM2 keyboard j/n
	-extend/retract telescoping sections - AXIS_CRANE_ARM3 keyboard lshift + j/n
	-tilt hydraulic jib/luffing jib down/up - AXIS_CRANE_ARM4 keyboard lshift + k/m
	-lower hook - AXIS_CRANE_TOOL keyboard lctrl + k/m
	-raise/lower y-guy brace - AXIS_FRONTLOADER_TOOL3 keyboard lshift + lctrl + j/n
	-spread/crowd y-guy brace - AXIS_FRONTLOADER_TOOL4 keyboard lshift + lctrl + k/m
	-fold (hide/unhide cables and/or lattice if configured) - keyboard x